,b3##LENGTH##MILLIMETERS,b2##LENGTH##MILLIMETERS,b1##LENGTH##MILLIMETERS,Weight##LENGTH##MILLIMETERS,WarrantyStartDate##OTHER##,WarrantyGuarantorParts##OTHER##,WarrantyGuarantorLabor##OTHER##,WarrantyDurationUnit##OTHER##,WarrantyDurationParts##OTHER##,WarrantyDurationLabor##OTHER##,WarrantyDescription##OTHER##,WallOuterLeaf##LENGTH##MILLIMETERS,WallInnerLeafRange##OTHER##,WallInnerLeaf##LENGTH##MILLIMETERS,WallCavity##LENGTH##MILLIMETERS,Version##OTHER##,Uniclass2015##OTHER##,URL##OTHER##,Type Comments##OTHER##,ThermalTransmittance##LENGTH##MILLIMETERS,TagNumber##OTHER##,TSE_Version##OTHER##,TSE_TechnicalContact##OTHER##,TSE_SalesContact##OTHER##,TSE_Revision##OTHER##,TSE_QR code##OTHER##,TSE_ProductGuid##OTHER##,TSE_ProductCertification##OTHER##,TSE_Model##OTHER##,TSE_ManufacturerURL##OTHER##,TSE_InstallationInstructions##OTHER##,TSE_EAN_code##OTHER##,TSE_Documentation##OTHER##,TSE_Description##OTHER##,TSE_Classification##OTHER##,TSE_BIMObjectSource##OTHER##,TSE_BIMObjectName##OTHER##,SustainabilityPerformance##OTHER##,Status##OTHER##,Standard##OTHER##,Span##LENGTH##MILLIMETERS,Slope##LENGTH##MILLIMETERS,Sizes##OTHER##,Size##OTHER##,Shape##OTHER##,SerialNumber##OTHER##,SafeWorkingLoad##LENGTH##MILLIMETERS,Roll##LENGTH##MILLIMETERS,Revision##OTHER##,ReplacementCost##OTHER##,Reference##OTHER##,ProductInformation##OTHER##,NominalWidth##LENGTH##MILLIMETERS,NominalLength##LENGTH##MILLIMETERS,NominalHeight##LENGTH##MILLIMETERS,Name##OTHER##,NBSTypeID##OTHER##,NBSReference##OTHER##,NBSDescription##OTHER##,ModelReference##OTHER##,ModelNumber##OTHER##,MinLintelLength##OTHER##,MaxLintelLength##OTHER##,MaterialFinishAndCoatingReference##OTHER##,Material##OTHER##,ManufacturerURL##OTHER##,Manufacturer##OTHER##,LoadCategory##OTHER##,LoadBearing##OTHER##,LintelType##OTHER##,LintelTop##LENGTH##MILLIMETERS,LintelThickness##LENGTH##MILLIMETERS,LintelOuterLeaf##LENGTH##MILLIMETERS,LintelMaterial##OTHER##,Model##OTHER##,LintelLip##LENGTH##MILLIMETERS,LintelLength##LENGTH##MILLIMETERS,LintelInsulation##OTHER##,LintelInnerLeaf##LENGTH##MILLIMETERS,LintelHeight##LENGTH##MILLIMETERS,LintelFace##LENGTH##MILLIMETERS,LintelCavity##LENGTH##MILLIMETERS,LengthIncrement##OTHER##,Keynote##OTHER##,IsExternal##OTHER##,InstallationDate##OTHER##,IfcExportType##OTHER##,IfcExportAs##OTHER##,Grade##OTHER##,FireRating##OTHER##,Finish##OTHER##,Features##OTHER##,ExpectedLife##OTHER##,EndBearing##LENGTH##MILLIMETERS,DurationUnit##OTHER##,Description##OTHER##,CreatedOn##OTHER##,CreatedBy##OTHER##,Constituents##OTHER##,Color##OTHER##,CodePerformance##OTHER##,ClearSpan##LENGTH##MILLIMETERS,CharacteristicThermalConductivity##LENGTH##MILLIMETERS,CharacteristicResistanceToFire##LENGTH##MILLIMETERS,CharacteristicDeflectionUnderLoad##LENGTH##MILLIMETERS,WallCavityRange##OTHER##,Category##OTHER##,BarCode##OTHER##,BIMObjectName##OTHER##,Author##OTHER##,AssetType##OTHER##,AssetIdentifier##OTHER##,Assembly Code##OTHER##,AllowableLoadLimiting##LENGTH##MILLIMETERS,AccessibilityPerformance##OTHER##
TataSteel_Lintel_CG50_125_900,22.100000000000,147.100000000000,117.100000000000,6.400000000000,1900-12-31T23:59:59,n/a,n/a,n/a,n/a,n/a,n/a,102.000000000000,125-140,125.000000000000,50.000000000000,,Pr_20_85_48_11,www.catnic.com,,0.000000000000,n/a,,catnic.technical@tatasteel.com,catnic.sales@tatasteel.com,,<None>,,www.catnic.com,TataSteel_Lintel_CG50_125_900,www.catnic.com,www.catnic.com,,www.catnic.com,"Catnic CG lintels use unique, discrete brackets in place of a base.
Depending on the wall construction, they can have a linear thermal
transmittance ψ value of less than 0.21 W/mK.",,,TataSteel_Lintel_CG50_125_900,n/a,n/a,,600.000000000000,0.000000000000,,140H x264W x900L,Open back lintel,n/a,12.000000000000,0.000000000000,,n/a,,www.catnic.com,264.000000000000,900.000000000000,140.000000000000,Lintel,n/a,F30 755,Pre fabricated Steel Lintel,Cavity Walls,CG,750,"3600mm for a 100mm inner leaf. 
3000mm for a 125mm inner leaf",,Galvanised Steel,www.catnic.com,"Catnic, TATA",STANDARD DUTY,0,CAVITY,10.000000000000,1.600000000000,95.000000000000,Steel,TataSteel_Lintel_CG50_125_900,2.000000000000,900.000000000000,Insulation,125.000000000000,140.000000000000,46.000000000000,44.200000000000,"150mm up to 3000mm. 
300mm above 3000mm",,0,1900-12-31T23:59:59,LINTEL,IfcBeamType,DX51,60,Galv and Powder coated,n/a,60 yrs,150.000000000000,,Standard duty cavity wall lintel,,,,Black,n/a,600.000000000000,0.000000000000,60.000000000000,0.000000000000,50-65,n/a,n/a,TataSteel_Lintel_CG50_125_900,TATA,FIXED,n/a,,12.000000000000,n/a
TataSteel_Lintel_CG50_125_1200,22.100000000000,147.100000000000,117.100000000000,6.400000000000,1900-12-31T23:59:59,n/a,n/a,n/a,n/a,n/a,n/a,102.000000000000,125-140,125.000000000000,50.000000000000,,Pr_20_85_48_11,www.catnic.com,,0.000000000000,n/a,,catnic.technical@tatasteel.com,catnic.sales@tatasteel.com,,<None>,,www.catnic.com,TataSteel_Lintel_CG50_125_1200,www.catnic.com,www.catnic.com,,www.catnic.com,"Catnic CG lintels use unique, discrete brackets in place of a base.
Depending on the wall construction, they can have a linear thermal
transmittance ψ value of less than 0.21 W/mK.",,,TataSteel_Lintel_CG50_125_1200,n/a,n/a,,900.000000000000,0.000000000000,,140H x264W x1200L,Open back lintel,n/a,12.000000000000,0.000000000000,,n/a,,www.catnic.com,264.000000000000,1200.000000000000,140.000000000000,Lintel,n/a,F30 755,Pre fabricated Steel Lintel,Cavity Walls,CG,750,"3600mm for a 100mm inner leaf. 
3000mm for a 125mm inner leaf",,Galvanised Steel,www.catnic.com,"Catnic, TATA",STANDARD DUTY,0,CAVITY,10.000000000000,1.600000000000,95.000000000000,Steel,TataSteel_Lintel_CG50_125_1200,2.000000000000,1200.000000000000,Insulation,125.000000000000,140.000000000000,46.000000000000,44.200000000000,"150mm up to 3000mm. 
300mm above 3000mm",,0,1900-12-31T23:59:59,LINTEL,IfcBeamType,DX51,60,Galv and Powder coated,n/a,60 yrs,150.000000000000,,Standard duty cavity wall lintel,,,,Black,n/a,900.000000000000,0.000000000000,60.000000000000,0.000000000000,50-65,n/a,n/a,TataSteel_Lintel_CG50_125_1200,TATA,FIXED,n/a,,12.000000000000,n/a
TataSteel_Lintel_CG50_125_1500,22.500000000000,147.500000000000,117.500000000000,8.000000000000,1900-12-31T23:59:59,n/a,n/a,n/a,n/a,n/a,n/a,102.000000000000,125-140,125.000000000000,50.000000000000,,Pr_20_85_48_11,www.catnic.com,,0.000000000000,n/a,,catnic.technical@tatasteel.com,catnic.sales@tatasteel.com,,<None>,,www.catnic.com,TataSteel_Lintel_CG50_125_1500,www.catnic.com,www.catnic.com,,www.catnic.com,"Catnic CG lintels use unique, discrete brackets in place of a base.
Depending on the wall construction, they can have a linear thermal
transmittance ψ value of less than 0.21 W/mK.",,,TataSteel_Lintel_CG50_125_1500,n/a,n/a,,1200.000000000000,0.000000000000,,140H x265W x1500L,Open back lintel,n/a,17.000000000000,0.000000000000,,n/a,,www.catnic.com,265.000000000000,1500.000000000000,140.000000000000,Lintel,n/a,F30 755,Pre fabricated Steel Lintel,Cavity Walls,CG,750,"3600mm for a 100mm inner leaf. 
3000mm for a 125mm inner leaf",,Galvanised Steel,www.catnic.com,"Catnic, TATA",STANDARD DUTY,0,CAVITY,10.000000000000,2.000000000000,95.000000000000,Steel,TataSteel_Lintel_CG50_125_1500,2.000000000000,1500.000000000000,Insulation,125.000000000000,140.000000000000,46.000000000000,45.000000000000,"150mm up to 3000mm. 
300mm above 3000mm",,0,1900-12-31T23:59:59,LINTEL,IfcBeamType,DX51,60,Galv and Powder coated,n/a,60 yrs,150.000000000000,,Standard duty cavity wall lintel,,,,Black,n/a,1200.000000000000,0.000000000000,60.000000000000,0.000000000000,50-65,n/a,n/a,TataSteel_Lintel_CG50_125_1500,TATA,FIXED,n/a,,17.000000000000,n/a
TataSteel_Lintel_CG50_125_1800,22.500000000000,147.500000000000,117.500000000000,8.000000000000,1900-12-31T23:59:59,n/a,n/a,n/a,n/a,n/a,n/a,102.000000000000,125-140,125.000000000000,50.000000000000,,Pr_20_85_48_11,www.catnic.com,,0.000000000000,n/a,,catnic.technical@tatasteel.com,catnic.sales@tatasteel.com,,<None>,,www.catnic.com,TataSteel_Lintel_CG50_125_1800,www.catnic.com,www.catnic.com,,www.catnic.com,"Catnic CG lintels use unique, discrete brackets in place of a base.
Depending on the wall construction, they can have a linear thermal
transmittance ψ value of less than 0.21 W/mK.",,,TataSteel_Lintel_CG50_125_1800,n/a,n/a,,1500.000000000000,0.000000000000,,140H x265W x1800L,Open back lintel,n/a,17.000000000000,0.000000000000,,n/a,,www.catnic.com,265.000000000000,1800.000000000000,140.000000000000,Lintel,n/a,F30 755,Pre fabricated Steel Lintel,Cavity Walls,CG,750,"3600mm for a 100mm inner leaf. 
3000mm for a 125mm inner leaf",,Galvanised Steel,www.catnic.com,"Catnic, TATA",STANDARD DUTY,0,CAVITY,10.000000000000,2.000000000000,95.000000000000,Steel,TataSteel_Lintel_CG50_125_1800,2.000000000000,1800.000000000000,Insulation,125.000000000000,140.000000000000,46.000000000000,45.000000000000,"150mm up to 3000mm. 
300mm above 3000mm",,0,1900-12-31T23:59:59,LINTEL,IfcBeamType,DX51,60,Galv and Powder coated,n/a,60 yrs,150.000000000000,,Standard duty cavity wall lintel,,,,Black,n/a,1500.000000000000,0.000000000000,60.000000000000,0.000000000000,50-65,n/a,n/a,TataSteel_Lintel_CG50_125_1800,TATA,FIXED,n/a,,17.000000000000,n/a
TataSteel_Lintel_CG50_125_2100,22.500000000000,147.500000000000,117.500000000000,9.200000000000,1900-12-31T23:59:59,n/a,n/a,n/a,n/a,n/a,n/a,102.000000000000,125-140,125.000000000000,50.000000000000,,Pr_20_85_48_11,www.catnic.com,,0.000000000000,n/a,,catnic.technical@tatasteel.com,catnic.sales@tatasteel.com,,<None>,,www.catnic.com,TataSteel_Lintel_CG50_125_2100,www.catnic.com,www.catnic.com,,www.catnic.com,"Catnic CG lintels use unique, discrete brackets in place of a base.
Depending on the wall construction, they can have a linear thermal
transmittance ψ value of less than 0.21 W/mK.",,,TataSteel_Lintel_CG50_125_2100,n/a,n/a,,1800.000000000000,0.000000000000,,180H x265W x2100L,Open back lintel,n/a,20.000000000000,0.000000000000,,n/a,,www.catnic.com,265.000000000000,2100.000000000000,180.000000000000,Lintel,n/a,F30 755,Pre fabricated Steel Lintel,Cavity Walls,CG,750,"3600mm for a 100mm inner leaf. 
3000mm for a 125mm inner leaf",,Galvanised Steel,www.catnic.com,"Catnic, TATA",STANDARD DUTY,0,CAVITY,10.000000000000,2.000000000000,95.000000000000,Steel,TataSteel_Lintel_CG50_125_2100,2.000000000000,2100.000000000000,Insulation,125.000000000000,180.000000000000,85.000000000000,45.000000000000,"150mm up to 3000mm. 
300mm above 3000mm",,0,1900-12-31T23:59:59,LINTEL,IfcBeamType,DX51,60,Galv and Powder coated,n/a,60 yrs,150.000000000000,,Standard duty cavity wall lintel,,,,Black,n/a,1800.000000000000,0.000000000000,60.000000000000,0.000000000000,50-65,n/a,n/a,TataSteel_Lintel_CG50_125_2100,TATA,FIXED,n/a,,20.000000000000,n/a
TataSteel_Lintel_CG50_125_2400,22.500000000000,147.500000000000,117.500000000000,9.200000000000,1900-12-31T23:59:59,n/a,n/a,n/a,n/a,n/a,n/a,102.000000000000,125-140,125.000000000000,50.000000000000,,Pr_20_85_48_11,www.catnic.com,,0.000000000000,n/a,,catnic.technical@tatasteel.com,catnic.sales@tatasteel.com,,<None>,,www.catnic.com,TataSteel_Lintel_CG50_125_2400,www.catnic.com,www.catnic.com,,www.catnic.com,"Catnic CG lintels use unique, discrete brackets in place of a base.
Depending on the wall construction, they can have a linear thermal
transmittance ψ value of less than 0.21 W/mK.",,,TataSteel_Lintel_CG50_125_2400,n/a,n/a,,2100.000000000000,0.000000000000,,180H x265W x2400L,Open back lintel,n/a,20.000000000000,0.000000000000,,n/a,,www.catnic.com,265.000000000000,2400.000000000000,180.000000000000,Lintel,n/a,F30 755,Pre fabricated Steel Lintel,Cavity Walls,CG,750,"3600mm for a 100mm inner leaf. 
3000mm for a 125mm inner leaf",,Galvanised Steel,www.catnic.com,"Catnic, TATA",STANDARD DUTY,0,CAVITY,10.000000000000,2.000000000000,95.000000000000,Steel,TataSteel_Lintel_CG50_125_2400,2.000000000000,2400.000000000000,Insulation,125.000000000000,180.000000000000,85.000000000000,45.000000000000,"150mm up to 3000mm. 
300mm above 3000mm",,0,1900-12-31T23:59:59,LINTEL,IfcBeamType,DX51,60,Galv and Powder coated,n/a,60 yrs,150.000000000000,,Standard duty cavity wall lintel,,,,Black,n/a,2100.000000000000,0.000000000000,60.000000000000,0.000000000000,50-65,n/a,n/a,TataSteel_Lintel_CG50_125_2400,TATA,FIXED,n/a,,20.000000000000,n/a
TataSteel_Lintel_CG50_125_2700,23.000000000000,148.000000000000,118.000000000000,12.900000000000,1900-12-31T23:59:59,n/a,n/a,n/a,n/a,n/a,n/a,102.000000000000,125-140,125.000000000000,50.000000000000,,Pr_20_85_48_11,www.catnic.com,,0.000000000000,n/a,,catnic.technical@tatasteel.com,catnic.sales@tatasteel.com,,<None>,,www.catnic.com,TataSteel_Lintel_CG50_125_2700,www.catnic.com,www.catnic.com,,www.catnic.com,"Catnic CG lintels use unique, discrete brackets in place of a base.
Depending on the wall construction, they can have a linear thermal
transmittance ψ value of less than 0.21 W/mK.",,,TataSteel_Lintel_CG50_125_2700,n/a,n/a,,2400.000000000000,0.000000000000,,220H x266W x2700L,Open back lintel,n/a,26.000000000000,0.000000000000,,n/a,,www.catnic.com,266.000000000000,2700.000000000000,220.000000000000,Lintel,n/a,F30 755,Pre fabricated Steel Lintel,Cavity Walls,CG,750,"3600mm for a 100mm inner leaf. 
3000mm for a 125mm inner leaf",,Galvanised Steel,www.catnic.com,"Catnic, TATA",STANDARD DUTY,0,CAVITY,10.000000000000,2.500000000000,95.000000000000,Steel,TataSteel_Lintel_CG50_125_2700,2.000000000000,2700.000000000000,Insulation,125.000000000000,220.000000000000,122.000000000000,46.000000000000,"150mm up to 3000mm. 
300mm above 3000mm",,0,1900-12-31T23:59:59,LINTEL,IfcBeamType,DX51,60,Galv and Powder coated,n/a,60 yrs,150.000000000000,,Standard duty cavity wall lintel,,,,Black,n/a,2400.000000000000,0.000000000000,60.000000000000,0.000000000000,50-65,n/a,n/a,TataSteel_Lintel_CG50_125_2700,TATA,FIXED,n/a,,26.000000000000,n/a
TataSteel_Lintel_CG50_125_3000,23.000000000000,148.000000000000,118.000000000000,12.900000000000,1900-12-31T23:59:59,n/a,n/a,n/a,n/a,n/a,n/a,102.000000000000,125-140,125.000000000000,50.000000000000,,Pr_20_85_48_11,www.catnic.com,,0.000000000000,n/a,,catnic.technical@tatasteel.com,catnic.sales@tatasteel.com,,<None>,,www.catnic.com,TataSteel_Lintel_CG50_125_3000,www.catnic.com,www.catnic.com,,www.catnic.com,"Catnic CG lintels use unique, discrete brackets in place of a base.
Depending on the wall construction, they can have a linear thermal
transmittance ψ value of less than 0.21 W/mK.",,,TataSteel_Lintel_CG50_125_3000,n/a,n/a,,2700.000000000000,0.000000000000,,220H x266W x3000L,Open back lintel,n/a,26.000000000000,0.000000000000,,n/a,,www.catnic.com,266.000000000000,3000.000000000000,220.000000000000,Lintel,n/a,F30 755,Pre fabricated Steel Lintel,Cavity Walls,CG,750,"3600mm for a 100mm inner leaf. 
3000mm for a 125mm inner leaf",,Galvanised Steel,www.catnic.com,"Catnic, TATA",STANDARD DUTY,0,CAVITY,10.000000000000,2.500000000000,95.000000000000,Steel,TataSteel_Lintel_CG50_125_3000,2.000000000000,3000.000000000000,Insulation,125.000000000000,220.000000000000,122.000000000000,46.000000000000,"150mm up to 3000mm. 
300mm above 3000mm",,0,1900-12-31T23:59:59,LINTEL,IfcBeamType,DX51,60,Galv and Powder coated,n/a,60 yrs,150.000000000000,,Standard duty cavity wall lintel,,,,Black,n/a,2700.000000000000,0.000000000000,60.000000000000,0.000000000000,50-65,n/a,n/a,TataSteel_Lintel_CG50_125_3000,TATA,FIXED,n/a,,26.000000000000,n/a
