,URL##OTHER##,Type Comments##OTHER##,Manufacturer##OTHER##,LintelWidth##LENGTH##MILLIMETERS,h##LENGTH##MILLIMETERS,c##LENGTH##MILLIMETERS,b2##LENGTH##MILLIMETERS,b1##LENGTH##MILLIMETERS,b##LENGTH##MILLIMETERS,a##LENGTH##MILLIMETERS,Weight##LENGTH##MILLIMETERS,WarrantyStartDate##OTHER##,WarrantyGuarantorParts##OTHER##,WarrantyGuarantorLabor##OTHER##,WarrantyDurationUnit##OTHER##,WarrantyDurationParts##OTHER##,WarrantyDurationLabor##OTHER##,WarrantyDescription##OTHER##,Version##OTHER##,Uniclass2015##OTHER##,Type Image##OTHER##,LintelThickness##LENGTH##MILLIMETERS,ThermalTransmittance##LENGTH##MILLIMETERS,TagNumber##OTHER##,TSE_Version##OTHER##,TSE_TechnicalContact##OTHER##,TSE_SalesContact##OTHER##,TSE_Revision##OTHER##,TSE_QR code##OTHER##,TSE_ProductGuid##OTHER##,TSE_ProductCertification##OTHER##,TSE_Model##OTHER##,TSE_ManufacturerURL##OTHER##,TSE_InstallationInstructions##OTHER##,TSE_EAN_code##OTHER##,TSE_Documentation##OTHER##,TSE_Description##OTHER##,TSE_Classification##OTHER##,TSE_BIMObjectSource##OTHER##,TSE_BIMObjectName##OTHER##,SustainabilityPerformance##OTHER##,Steel##OTHER##,Status##OTHER##,Standard##OTHER##,Span##LENGTH##MILLIMETERS,Slope##LENGTH##MILLIMETERS,Sizes##OTHER##,Size##OTHER##,Shape##OTHER##,SerialNumber##OTHER##,SafeWorkingLoad##LENGTH##MILLIMETERS,Roll##LENGTH##MILLIMETERS,Revision##OTHER##,ReplacementCost##OTHER##,Reference##OTHER##,ProductInformation##OTHER##,NominalWidth##LENGTH##MILLIMETERS,NominalLength##LENGTH##MILLIMETERS,NominalHeight##LENGTH##MILLIMETERS,Name##OTHER##,NBSTypeID##OTHER##,NBSReference##OTHER##,NBSDescription##OTHER##,ModelReference##OTHER##,ModelNumber##OTHER##,Model##OTHER##,MinLintelLength##OTHER##,MaxLintelLength##OTHER##,MaterialFinishAndCoatingReference##OTHER##,ManufacturerURL##OTHER##,LoadCategory##OTHER##,LoadBearing##OTHER##,LintelType##OTHER##,WallThickness##LENGTH##MILLIMETERS,LintelLength##LENGTH##MILLIMETERS,LintelHeight##LENGTH##MILLIMETERS,LengthIncrement##OTHER##,Keynote##OTHER##,IsExternal##OTHER##,InstallationDate##OTHER##,IfcExportType##OTHER##,IfcExportAs##OTHER##,Grade##OTHER##,FireRating##OTHER##,Finish##OTHER##,Features##OTHER##,ExpectedLife##OTHER##,EndBearing##LENGTH##MILLIMETERS,DurationUnit##OTHER##,Description##OTHER##,CreatedOn##OTHER##,CreatedBy##OTHER##,Constituents##OTHER##,Color##OTHER##,CodePerformance##OTHER##,ClearSpan##LENGTH##MILLIMETERS,CharacteristicThermalConductivity##LENGTH##MILLIMETERS,CharacteristicResistanceToFire##LENGTH##MILLIMETERS,CharacteristicDeflectionUnderLoad##LENGTH##MILLIMETERS,Category##OTHER##,BarCode##OTHER##,BIMObjectName##OTHER##,Author##OTHER##,AssetType##OTHER##,AssetIdentifier##OTHER##,Assembly Code##OTHER##,AllowableLoadLimiting##LENGTH##MILLIMETERS,AccessibilityPerformance##OTHER##
TataSteel_Lintel_CN92_1050,www.catnic.com,,"Catnic, TATA",68.000000000000,25.000000000000,20.000000000000,37.500000000000,37.500000000000,10.000000000000,5.000000000000,1.200000000000,1900-12-31T23:59:59,n/a,n/a,n/a,n/a,n/a,n/a,,Pr_20_85_48_11,<None>,1.200000000000,0.000000000000,n/a,,catnic.technical@tatasteel.com,catnic.sales@tatasteel.com,,<None>,,www.catnic.com,TataSteel_Lintel_CN92_1050,www.catnic.com,www.catnic.com,,www.catnic.com,,,,TataSteel_Lintel_CN92_1050,n/a,Steel,n/a,,900.000000000000,0.000000000000,,25H x68W x1050L,Corrugated,n/a,7.000000000000,0.000000000000,,n/a,,www.catnic.com,68.000000000000,1050.000000000000,25.000000000000,Lintel,n/a,F30 755,Pre fabricated Steel Lintel,Internal Walls,CN92,TataSteel_Lintel_CN92_1050,1050,1200,,www.catnic.com,EXTRA LIGHT DUTY,1,SOLID INTERNAL,75.000000000000,1050.000000000000,25.000000000000,"150mm up to 3000mm. 
300mm above 3000mm",,0,1900-12-31T23:59:59,LINTEL,IfcBeamType,DX51,60,Galv and Powder coated,n/a,60 yrs,75.000000000000,,Extra light duty internal wall lintel,,,,Black,n/a,900.000000000000,0.000000000000,60.000000000000,0.000000000000,n/a,n/a,TataSteel_Lintel_CN92_1050,TATA,FIXED,n/a,,7.000000000000,n/a
TataSteel_Lintel_CN92_1200,www.catnic.com,,"Catnic, TATA",68.000000000000,25.000000000000,20.000000000000,37.500000000000,37.500000000000,10.000000000000,5.000000000000,1.200000000000,1900-12-31T23:59:59,n/a,n/a,n/a,n/a,n/a,n/a,,Pr_20_85_48_11,<None>,1.200000000000,0.000000000000,n/a,,catnic.technical@tatasteel.com,catnic.sales@tatasteel.com,,<None>,,www.catnic.com,TataSteel_Lintel_CN92_1200,www.catnic.com,www.catnic.com,,www.catnic.com,,,,TataSteel_Lintel_CN92_1200,n/a,Steel,n/a,,1050.000000000000,0.000000000000,,25H x68W x1200L,Corrugated,n/a,7.000000000000,0.000000000000,,n/a,,www.catnic.com,68.000000000000,1200.000000000000,25.000000000000,Lintel,n/a,F30 755,Pre fabricated Steel Lintel,Internal Walls,CN92,TataSteel_Lintel_CN92_1200,1050,1200,,www.catnic.com,EXTRA LIGHT DUTY,1,SOLID INTERNAL,75.000000000000,1200.000000000000,25.000000000000,"150mm up to 3000mm. 
300mm above 3000mm",,0,1900-12-31T23:59:59,LINTEL,IfcBeamType,DX51,60,Galv and Powder coated,n/a,60 yrs,75.000000000000,,Extra light duty internal wall lintel,,,,Black,n/a,1050.000000000000,0.000000000000,60.000000000000,0.000000000000,n/a,n/a,TataSteel_Lintel_CN92_1200,TATA,FIXED,n/a,,7.000000000000,n/a
