,ro##LENGTH##MILLIMETERS,r##LENGTH##MILLIMETERS,b3##LENGTH##MILLIMETERS,b2##LENGTH##MILLIMETERS,b1##LENGTH##MILLIMETERS,Weight##LENGTH##MILLIMETERS,WarrantyStartDate##OTHER##,WarrantyGuarantorParts##OTHER##,WarrantyGuarantorLabor##OTHER##,WarrantyDurationUnit##OTHER##,WarrantyDurationParts##OTHER##,WarrantyDurationLabor##OTHER##,WarrantyDescription##OTHER##,WallInnerLeafRange##OTHER##,WallCavityRange##OTHER##,Version##OTHER##,Uniclass2015##OTHER##,URL##OTHER##,Type Image##OTHER##,Type Comments##OTHER##,Manufacturer##OTHER##,LintelThickness##LENGTH##MILLIMETERS,ThermalTransmittance##LENGTH##MILLIMETERS,TagNumber##OTHER##,TSE_Version##OTHER##,TSE_TechnicalContact##OTHER##,TSE_SalesContact##OTHER##,TSE_Revision##OTHER##,TSE_QR code##OTHER##,TSE_ProductGuid##OTHER##,TSE_ProductCertification##OTHER##,TSE_Model##OTHER##,TSE_ManufacturerURL##OTHER##,TSE_InstallationInstructions##OTHER##,TSE_EAN_code##OTHER##,TSE_Documentation##OTHER##,TSE_Description##OTHER##,TSE_Classification##OTHER##,TSE_BIMObjectSource##OTHER##,TSE_BIMObjectName##OTHER##,SustainabilityPerformance##OTHER##,Steel##OTHER##,Status##OTHER##,Standard##OTHER##,Span##LENGTH##MILLIMETERS,Slope##LENGTH##MILLIMETERS,Sizes##OTHER##,Size##OTHER##,Shape##OTHER##,SerialNumber##OTHER##,SafeWorkingLoad##LENGTH##MILLIMETERS,Roll##LENGTH##MILLIMETERS,Revision##OTHER##,ReplacementCost##OTHER##,Reference##OTHER##,ProductInformation##OTHER##,WallOuterLeaf##LENGTH##MILLIMETERS,NominalWidth##LENGTH##MILLIMETERS,NominalLength##LENGTH##MILLIMETERS,NominalHeight##LENGTH##MILLIMETERS,Name##OTHER##,NBSTypeID##OTHER##,NBSReference##OTHER##,NBSDescription##OTHER##,ModelReference##OTHER##,ModelNumber##OTHER##,Model##OTHER##,MinLintelLength##OTHER##,MaxLintelLength##OTHER##,MaterialFinishAndCoatingReference##OTHER##,ManufacturerURL##OTHER##,LoadCategory##OTHER##,LoadBearing##OTHER##,LintelType##OTHER##,LintelOuterLeaf##LENGTH##MILLIMETERS,LintelLength##LENGTH##MILLIMETERS,LintelHeight##LENGTH##MILLIMETERS,LintelCavity##LENGTH##MILLIMETERS,LengthIncrement##OTHER##,Keynote##OTHER##,IsExternal##OTHER##,InstallationDate##OTHER##,WallInnerLeaf##LENGTH##MILLIMETERS,IfcExportType##OTHER##,IfcExportAs##OTHER##,Grade##OTHER##,FireRating##OTHER##,Finish##OTHER##,Features##OTHER##,ExpectedLife##OTHER##,EndBearing##LENGTH##MILLIMETERS,DurationUnit##OTHER##,Description##OTHER##,CreatedOn##OTHER##,CreatedBy##OTHER##,Constituents##OTHER##,Color##OTHER##,CodePerformance##OTHER##,ClearSpan##LENGTH##MILLIMETERS,CharacteristicThermalConductivity##LENGTH##MILLIMETERS,CharacteristicResistanceToFire##LENGTH##MILLIMETERS,CharacteristicDeflectionUnderLoad##LENGTH##MILLIMETERS,WallCavity##LENGTH##MILLIMETERS,Category##OTHER##,BarCode##OTHER##,BIMObjectName##OTHER##,Author##OTHER##,AssetType##OTHER##,AssetIdentifier##OTHER##,LintelInnerLeaf##LENGTH##MILLIMETERS,Assembly Code##OTHER##,AllowableLoadLimiting##LENGTH##MILLIMETERS,AccessibilityPerformance##OTHER##
TataSteel_Lintel_CN51C_1950,8.100000000000,5.000000000000,5.000000000000,105.000000000000,107.000000000000,16.000000000000,1900-12-31T23:59:59,n/a,n/a,n/a,n/a,n/a,n/a,N/A,N/A,,Pr_20_85_48_11,www.catnic.com,<None>,,"Catnic, TATA",3.100000000000,0.000000000000,n/a,,catnic.technical@tatasteel.com,catnic.sales@tatasteel.com,,<None>,,www.catnic.com,TataSteel_Lintel_CN51C_1950,www.catnic.com,www.catnic.com,,www.catnic.com,,,,TataSteel_Lintel_CN51C_1950,n/a,Steel,n/a,,1650.000000000000,0.000000000000,,167H x182W x1950L,Inverted T,n/a,12.700000000000,0.000000000000,,n/a,,www.catnic.com,102.000000000000,182.000000000000,1950.000000000000,167.000000000000,Lintel,n/a,F30 755,Pre fabricated Steel Lintel,External Solid Walls,CN50/CN51,TataSteel_Lintel_CN51C_1950,750,"1800 (CN50C)
 2700 (CN51C)",,www.catnic.com,STANDARD DUTY,1,SOLID EXTERNAL,91.000000000000,1950.000000000000,167.000000000000,6.200000000000,"150mm up to 3000mm. 
300mm above 3000mm",,1,1900-12-31T23:59:59,100.000000000000,LINTEL,IfcBeamType,DX51,60,Galv and Powder coated,n/a,60 yrs,150.000000000000,,External solid wall lintel,,,,Black,n/a,1650.000000000000,0.000000000000,60.000000000000,0.000000000000,10.000000000000,n/a,n/a,TataSteel_Lintel_CN51C_1950,TATA,FIXED,n/a,91.000000000000,,12.700000000000,n/a
TataSteel_Lintel_CN51C_2100,8.100000000000,5.000000000000,5.000000000000,105.000000000000,107.000000000000,16.000000000000,1900-12-31T23:59:59,n/a,n/a,n/a,n/a,n/a,n/a,N/A,N/A,,Pr_20_85_48_11,www.catnic.com,<None>,,"Catnic, TATA",3.100000000000,0.000000000000,n/a,,catnic.technical@tatasteel.com,catnic.sales@tatasteel.com,,<None>,,www.catnic.com,TataSteel_Lintel_CN51C_2100,www.catnic.com,www.catnic.com,,www.catnic.com,,,,TataSteel_Lintel_CN51C_2100,n/a,Steel,n/a,,1800.000000000000,0.000000000000,,167H x182W x2100L,Inverted T,n/a,12.700000000000,0.000000000000,,n/a,,www.catnic.com,102.000000000000,182.000000000000,2100.000000000000,167.000000000000,Lintel,n/a,F30 755,Pre fabricated Steel Lintel,External Solid Walls,CN50/CN51,TataSteel_Lintel_CN51C_2100,750,"1800 (CN50C)
 2700 (CN51C)",,www.catnic.com,STANDARD DUTY,1,SOLID EXTERNAL,91.000000000000,2100.000000000000,167.000000000000,6.200000000000,"150mm up to 3000mm. 
300mm above 3000mm",,1,1900-12-31T23:59:59,100.000000000000,LINTEL,IfcBeamType,DX51,60,Galv and Powder coated,n/a,60 yrs,150.000000000000,,External solid wall lintel,,,,Black,n/a,1800.000000000000,0.000000000000,60.000000000000,0.000000000000,10.000000000000,n/a,n/a,TataSteel_Lintel_CN51C_2100,TATA,FIXED,n/a,91.000000000000,,12.700000000000,n/a
TataSteel_Lintel_CN51C_2250,8.100000000000,5.000000000000,5.000000000000,105.000000000000,107.000000000000,16.000000000000,1900-12-31T23:59:59,n/a,n/a,n/a,n/a,n/a,n/a,N/A,N/A,,Pr_20_85_48_11,www.catnic.com,<None>,,"Catnic, TATA",3.100000000000,0.000000000000,n/a,,catnic.technical@tatasteel.com,catnic.sales@tatasteel.com,,<None>,,www.catnic.com,TataSteel_Lintel_CN51C_2250,www.catnic.com,www.catnic.com,,www.catnic.com,,,,TataSteel_Lintel_CN51C_2250,n/a,Steel,n/a,,1950.000000000000,0.000000000000,,167H x182W x2250L,Inverted T,n/a,12.700000000000,0.000000000000,,n/a,,www.catnic.com,102.000000000000,182.000000000000,2250.000000000000,167.000000000000,Lintel,n/a,F30 755,Pre fabricated Steel Lintel,External Solid Walls,CN50/CN51,TataSteel_Lintel_CN51C_2250,750,"1800 (CN50C)
 2700 (CN51C)",,www.catnic.com,STANDARD DUTY,1,SOLID EXTERNAL,91.000000000000,2250.000000000000,167.000000000000,6.200000000000,"150mm up to 3000mm. 
300mm above 3000mm",,1,1900-12-31T23:59:59,100.000000000000,LINTEL,IfcBeamType,DX51,60,Galv and Powder coated,n/a,60 yrs,150.000000000000,,External solid wall lintel,,,,Black,n/a,1950.000000000000,0.000000000000,60.000000000000,0.000000000000,10.000000000000,n/a,n/a,TataSteel_Lintel_CN51C_2250,TATA,FIXED,n/a,91.000000000000,,12.700000000000,n/a
TataSteel_Lintel_CN51C_2400,8.100000000000,5.000000000000,5.000000000000,105.000000000000,107.000000000000,16.000000000000,1900-12-31T23:59:59,n/a,n/a,n/a,n/a,n/a,n/a,N/A,N/A,,Pr_20_85_48_11,www.catnic.com,<None>,,"Catnic, TATA",3.100000000000,0.000000000000,n/a,,catnic.technical@tatasteel.com,catnic.sales@tatasteel.com,,<None>,,www.catnic.com,TataSteel_Lintel_CN51C_2400,www.catnic.com,www.catnic.com,,www.catnic.com,,,,TataSteel_Lintel_CN51C_2400,n/a,Steel,n/a,,2100.000000000000,0.000000000000,,167H x182W x2400L,Inverted T,n/a,12.700000000000,0.000000000000,,n/a,,www.catnic.com,102.000000000000,182.000000000000,2400.000000000000,167.000000000000,Lintel,n/a,F30 755,Pre fabricated Steel Lintel,External Solid Walls,CN50/CN51,TataSteel_Lintel_CN51C_2400,750,"1800 (CN50C)
 2700 (CN51C)",,www.catnic.com,STANDARD DUTY,1,SOLID EXTERNAL,91.000000000000,2400.000000000000,167.000000000000,6.200000000000,"150mm up to 3000mm. 
300mm above 3000mm",,1,1900-12-31T23:59:59,100.000000000000,LINTEL,IfcBeamType,DX51,60,Galv and Powder coated,n/a,60 yrs,150.000000000000,,External solid wall lintel,,,,Black,n/a,2100.000000000000,0.000000000000,60.000000000000,0.000000000000,10.000000000000,n/a,n/a,TataSteel_Lintel_CN51C_2400,TATA,FIXED,n/a,91.000000000000,,12.700000000000,n/a
TataSteel_Lintel_CN51C_2550,8.100000000000,5.000000000000,5.000000000000,105.000000000000,107.000000000000,16.000000000000,1900-12-31T23:59:59,n/a,n/a,n/a,n/a,n/a,n/a,N/A,N/A,,Pr_20_85_48_11,www.catnic.com,<None>,,"Catnic, TATA",3.100000000000,0.000000000000,n/a,,catnic.technical@tatasteel.com,catnic.sales@tatasteel.com,,<None>,,www.catnic.com,TataSteel_Lintel_CN51C_2550,www.catnic.com,www.catnic.com,,www.catnic.com,,,,TataSteel_Lintel_CN51C_2550,n/a,Steel,n/a,,2250.000000000000,0.000000000000,,167H x182W x2550L,Inverted T,n/a,12.700000000000,0.000000000000,,n/a,,www.catnic.com,102.000000000000,182.000000000000,2550.000000000000,167.000000000000,Lintel,n/a,F30 755,Pre fabricated Steel Lintel,External Solid Walls,CN50/CN51,TataSteel_Lintel_CN51C_2550,750,"1800 (CN50C)
 2700 (CN51C)",,www.catnic.com,STANDARD DUTY,1,SOLID EXTERNAL,91.000000000000,2550.000000000000,167.000000000000,6.200000000000,"150mm up to 3000mm. 
300mm above 3000mm",,1,1900-12-31T23:59:59,100.000000000000,LINTEL,IfcBeamType,DX51,60,Galv and Powder coated,n/a,60 yrs,150.000000000000,,External solid wall lintel,,,,Black,n/a,2250.000000000000,0.000000000000,60.000000000000,0.000000000000,10.000000000000,n/a,n/a,TataSteel_Lintel_CN51C_2550,TATA,FIXED,n/a,91.000000000000,,12.700000000000,n/a
TataSteel_Lintel_CN51C_2700,8.100000000000,5.000000000000,5.000000000000,105.000000000000,107.000000000000,16.000000000000,1900-12-31T23:59:59,n/a,n/a,n/a,n/a,n/a,n/a,N/A,N/A,,Pr_20_85_48_11,www.catnic.com,<None>,,"Catnic, TATA",3.100000000000,0.000000000000,n/a,,catnic.technical@tatasteel.com,catnic.sales@tatasteel.com,,<None>,,www.catnic.com,TataSteel_Lintel_CN51C_2700,www.catnic.com,www.catnic.com,,www.catnic.com,,,,TataSteel_Lintel_CN51C_2700,n/a,Steel,n/a,,2400.000000000000,0.000000000000,,167H x182W x2700L,Inverted T,n/a,12.700000000000,0.000000000000,,n/a,,www.catnic.com,102.000000000000,182.000000000000,2700.000000000000,167.000000000000,Lintel,n/a,F30 755,Pre fabricated Steel Lintel,External Solid Walls,CN50/CN51,TataSteel_Lintel_CN51C_2700,750,"1800 (CN50C)
 2700 (CN51C)",,www.catnic.com,STANDARD DUTY,1,SOLID EXTERNAL,91.000000000000,2700.000000000000,167.000000000000,6.200000000000,"150mm up to 3000mm. 
300mm above 3000mm",,1,1900-12-31T23:59:59,100.000000000000,LINTEL,IfcBeamType,DX51,60,Galv and Powder coated,n/a,60 yrs,150.000000000000,,External solid wall lintel,,,,Black,n/a,2400.000000000000,0.000000000000,60.000000000000,0.000000000000,10.000000000000,n/a,n/a,TataSteel_Lintel_CN51C_2700,TATA,FIXED,n/a,91.000000000000,,12.700000000000,n/a
